NOTE:

1. Do not make any additional ‘.txt’ file
2. Regarding the simulation data index, first letter of the simulation index must have lower order than ‘c’ ex) A1, A2…. <-- not allowed. V120I10…. <-- allowed.
3. To change delay time or pulse width or both of gate signal in SIMetrix simulation, global variable T1, T2, T3 in python code should be changed according to pulse setting.